SELECTOR LEVER COMPONENT REMOVAL/INSTALLATION

id051800800800

1. Disconnect the negative battery cable.

2. To remove the interlock cable, remove the following parts.

  (1) Column cover (See COLUMN COVER REMOVAL/INSTALLATION.)

  (2) Driver side under panel

  (3) Accelerator pedal (See ACCELERATOR PEDAL REMOVAL/INSTALLATION [MZI-3.7].)

3. To remove the selector cable, remove the following parts.

  (1) Battery and battery tray

  (2) Air cleaner component (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [MZI-3.7].)

  (3) Dashboard (See DASHBOARD REMOVAL/INSTALLATION.)

  (4) Front A/C unit (See FRONT A/C UNIT REMOVAL/INSTALLATION.)

4. To remove the selector lever, remove the following parts.

  (1) Console (See CONSOLE REMOVAL/INSTALLATION.)

5. Remove in the order shown in the figure.

6. Install in the reverse order of removal.

L.H.D.

ac9uuw00001588

R.H.D.

ac9wzw00000035

1 | Clip
2 | Clip
3 | Clip
4 | Lock unit connector
5 | Interlock cable (SeeInterlock Cable Installation Note.)
6 | Clip
7 | Clip
8 | Selector cable (SeeSelector Cable Removal Note.) (SeeSelector Cable Installation Note.)
9 | Selector lever component connector
10 | Selector lever component
11 | Selector lever knob
12 | Selector lever panel
13 | Selector lever

Selector Cable Removal Note

1. Remove the clip.

2. Remove the selector cable.

ac9uuw00001591

3. Remove the selector cable from the cable bracket.

ac9uuw00001592

Selector Cable Installation Note

1. Install the selector cable and clip to the bracket as shown in the figure.

ac9uuw00001593

  Note
  • Steps 2 and 3 are for the selector cable replacement only.

2. Verify that the selector lever is in the P position.

3. Lock the lock piece of the selector cable (selector lever side) in the order shown in the figure.

L.H.D.

ac9wzw00000019

R.H.D.

ac9wzw00000020

4. Verify that the manual shaft is in the P position.

  Caution
  • Bending the selector cable in the manner shown in the figure will damage the cable and it may become loose when shifted. When installing the selector cable, hold it straight.

  ac9uuw00001595

5. Install the clip as shown in the figure.

ac9uuw00001596

ac9uuw00001597

  Note
  • Install the selector lever to the manual shaft lever with the clip side of the selector cable end facing up.

6. Install the selector lever to the manual shaft lever so that no load acts on the selector cable.

7. Confirm that the tip of the manual shaft lever projects out of the end of the selector cable.

8. Securely install the selector cable to the selector cable bracket.

Interlock Cable Installation Note

1. Push the interlock cable.

ac9uuw00001598

2. Verify that the marking on the slider pin is positioned as shown in the figure.

L.H.D.

ac9uuw00001599

R.H.D.

ac9wzw00000029

3. Push a 1.5mm {0.059 in} round bar or similar into hole A by fully pushing the slider pin in.

ac9uuw00001600

4. Fully pull the end of the interlock cable.

ac9uuw00001601

5. Push a 1.5mm {0.059 in} round bar or similar into hole B and hole C of the lock unit until it passes through.

ac9uuw00001600

6. Disconnect the brake switch connector.

7. Remove the brake switch. (See BRAKE PEDAL REMOVAL/INSTALLATION [L.H.D.].)(See BRAKE PEDAL REMOVAL/INSTALLATION [R.H.D.].)

8. Install a new brake switch. (See BRAKE PEDAL REMOVAL/INSTALLATION [L.H.D.].)(See BRAKE PEDAL REMOVAL/INSTALLATION [R.H.D.].)

  Caution
  • Do not connect the brake switch connector until the interlock cable is installed.

9. With the slider pin pressed, slide the lock unit to fix the lock unit hook into the bracket hole securely as shown in the figure.

ac9uuw00001602

  Caution
  • Allowing the interlock cable to be bent or twisted during installation can affect the lock unit operation.

10. Rotate the slider pin to release the lock and verify that it slides freely.

11. Pull the slider pin outward until it contacts the brake pedal stopper rubber and rotate the slider pin to lock.

ac9wzw00000030

12. Verify that the selector lever in the P position.

13. Install the interlock cable end to the cam pin on the selector lever.

L.H.D.

ac9wzw00000605

R.H.D

ac9wzw00000606

14. Fit the interlock cable in the U–groove in the selector lever base plate and install the clip.

15. Press the interlock cable lock piece in until it is locked.

ac9uuw00001604

  Caution
  • Applying a load to the interlock cable while pressing the lock piece in can affect the lock unit operation.

16. Remove a 1.5mm {0.059 in} round bar or similar from the lock unit holes A, B, and C.

ac9uuw00001600

17. Connect the brake switch connector with the brake pedal released.

  Caution
  • The clearance between the brake switch and the brake pedal is automatically adjusted to the correct amount when the brake switch connector is connected after the brake switch has been properly installed. If the brake switch is not properly installed or the connector is connected before installation, the clearance may be incorrect, causing a brake light malfunction. Therefore, always verify that the brake switch is properly installed before connecting the connector.
  • Once the brake switch clearance has automatically been adjusted, it cannot be adjusted again. Therefore, replace the switch with a new one when replacing the power brake unit or the pedal, or performing any procedure that changes the pedal stroke.

18. Turn the ignition switch to ON position.

19. Install the interlock cable to the steering lock.

20. Slide the outer casing to the steering lock and insert the clip over the convex part of the outer casing.

ac9uuw00001605