BLIND SPOT MONITORING (BSM) OFF INDICATOR LIGHT CONSTRUCTION/OPERATION [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE]

id0922009990e1

• Equipped in the instrument cluster.
• LEDs with low-power consumption and high durability have been adopted.
• Illuminates for approx. 3 s after the ignition switch is turned to the ON position to perform a bulb check.
• According to the signal from the BSM control module, illuminates when the BSM is turned off, and turns off when the BSM is operable.
• Flashes when a malfunction or loss of function is detected in the BSM to indicate that the BSM has a malfunction.
• Refer to BLIND SPOT MONITORING (BSM) OPERATION for the illumination/flash condition of the BSM OFF indicator light. (See BLIND SPOT MONITORING (BSM) OPERATION [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].)