LOWER PANEL REMOVAL/INSTALLATION

id091700801100

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Decoration panel (Driver side) (See DECORATION PANEL REMOVAL/INSTALLATION.)

  (2) Dashboard under cover (Driver side) (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

  (3) Side wall (See SIDE WALL REMOVAL/INSTALLATION.)

  (4) Console panel (LH) (See CONSOLE PANEL REMOVAL/INSTALLATION.)

  (5) Bonnet release lever (See BONNET LATCH AND RELEASE LEVER REMOVAL/INSTALLATION.)

  (6) Fuel-filler lid release lever (R.H.D.) (See FUEL-FILLER LID OPENER REMOVAL/INSTALLATION.)

  (7) Car-navigation unit (with car-navigation system) (See CAR-NAVIGATION UNIT REMOVAL/INSTALLATION.)

  (8) Parking sensor switch/indicator (with parking sensor system) (See PARKING SENSOR SWITCH/INDICATOR REMOVAL/INSTALLATION.)

  (9) Cluster switch (See CLUSTER SWITCH REMOVAL/INSTALLATION.)

3. Remove the screw.

R.H.D.

ac9wzw00002863

L.H.D.

ac9wzw00002864

4. Detach clips A and hook B by pulling them in the direction of the arrow.

5. Remove the hook B.

6. Disconnect the cabin temperature sensor connector and air hose.

7. Remove the lower panel.

8. Install in the reverse order of removal.