STEERING LOCK UNIT ID CODE REGISTRATION [ADVANCED KEYLESS ENTRY AND START SYSTEM]

id0914008073z6

  Caution
  • Do not place the following devices in the vehicle while programming, otherwise programming cannot be performed.
    ― M-MDS
    ― Personal computer
    ― Device that can send/receive radio waves

  Note
  • The steering lock unit and steering lock component are a single unit. Therefore, replace the steering lock component when replacing steering lock unit. (See STEERING WHEEL AND COLUMN REMOVAL/INSTALLATION.)
  • For this procedure, a programmed card key is necessary. If there is no programmed card key, perform the steering lock unit programming after the card key programming.

1. Bring the programmed card key into the vehicle.

2. Fully lower the driver-side door glass.

3. Connect the M-MDS to the DLC-2.

ac9uuw00000452

4. Pull out the M-MDS cable from the door glass opening and set the M-MDS outside the vehicle.

  Caution
  • Protect the cable and body contact area with a clean rag, otherwise they could be damaged.

5. After the vehicle is identified, select the following items from the initialization screen of the M-MDS.

  1. Select “Body”.
  2. Select “Security”.

6. Then, select items from the screen menu in the following order.

  1. Select “PATS Functions”.
  2. Select “Steering Lock Unit Programming”.

7. The security access begins and the M-MDS displays “OUT-CODE”.

  Note
  • When “OUT-CODE” is first displayed, turning the ignition switch from the OFF to the ON position 5 times will change the “OUT-CODE”.

8. Input the “IN-CODE” that corresponds to the “OUT-CODE” displayed on the M-MDS screen.

9. Perform procedures according to the directions on the M-MDS screen.