REAR OIL SEAL REPLACEMENT [MZI-3.7]

id0110c5800900

1. Remove the automatic transaxle. (See AUTOMATIC TRANSAXLE REMOVAL/INSTALLATION [AY6A-EL, AY6AX-EL].)

2. Remove the drive plate. (See DRIVE PLATE REMOVAL/INSTALLATION [AY6A-EL, AY6AX-EL].)

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

ac9wzw00002241

1 | CKP sensor pulse wheel
2 | Rear oil seal (See Rear Oil Seal Removal Note.) (See Rear Oil Seal Installation Note.)

Rear Oil Seal Removal Note

1. Using a flathead screwdriver, remove the rear oil seal.

ac9wzw00002242

Rear Oil Seal Installation Note

  Note
  • Lubricate the rear oil seal lips and bore with clean engine oil.

1. Push the rear oil seal slightly in by hand.

2. Tap the rear oil seal in evenly using the SST and a hammer.

ac9wzw00002243

  Substitution SST

  • 49 W011 101
  Outer diameter: 105 mm {4.13 in} or more
  Inner diameter: 93—105 mm {3.7—4.1 in}
  Tube with board thickness 2 mm {0.079 in} or more