POWER WINDOW MAIN SWITCH REMOVAL/INSTALLATION

id091200002000

1. Disconnect the negative battery cable.

2. Remove the inner garnish. (driver-side) (See INNER GARNISH REMOVAL/INSTALLATION.)

3. Remove the front door trim. (driver-side) (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)

4. Remove the screw, and remove the power window main switch from inside the front door trim.

ac9wzw00001641

5. Install in the reverse order of removal.