REAR SASH MOLDING REMOVAL

id091600805100

  Warning
  • Using a razor with bare hands can cause injury. Always wear gloves when using a razor.

1. Press tab C in the direction of the arrow and remove it.

ac9uuw00000652

2. While cutting the double-sided adhesive tape using a flathead screwdriver or a razor, separate the rear sash molding from the body.

3. Remove the tab D.

4. Rotate the rear sash molding in the direction of the arrow and remove tab A.

5. Rotate the rear sash molding in the direction of the arrow and remove tab B.

6. Remove the rear sash molding.