ON-BOARD DIAGNOSTIC SYSTEM PID/DATA MONITOR FUNCTION [AY6A-EL, AY6AX-EL]

id0502k1280600

Special Features

• The PID/DATA monitor function can monitor control data such as input signals/internal calculation values/output signals using the Mazda Modular Diagnostic System (M-MDS).

PID/DATA Monitor Table

Item | Definition | Unit/Operation
--- | --- | ---
BOO | Brake switch | On/Off
DWN_SW | Down switch | On/Off
ECT | ECT | °C {°F}
ENG_TORQ | Engine torque | N·m {kgf·cm, in·lbf}
GEAR_RA | Gear ratio | –
GEAR_SEL | Calculated gear range in TCM | 1st/2nd/3rd/4th/5th/6th
LOAD | Engine load | %
LPS | Pressure control solenoid | A
MNL SW | M position switch | On/Off
OSS | Output shaft speed | RPM
PNP | Park/Neutral | On/Off
RPM | Engine speed | RPM
SSA | Shift solenoid A | On/Off
SSB | Shift solenoid B | On/Off
SSC | Shift solenoid C | A
SSD | Shift solenoid D | A
SSE | Shift solenoid E | A
SSF | Shift solenoid F | A
TCCC | TCC control solenoid | A
TFT | ATF temperature | °C {°F}
TFTV | ATF temperature signal voltage | V
THOP | Throttle position | %
TR | TR switch | P/R/N/D/M
TRD | TR switch [D position] | On/Off
TRR | TR switch [R position] | On/Off
TSS | Input/turbine speed sensor | RPM
UP_SW | Up switch | On/Off
VPWR | Module supply voltage | V
VSS | Vehicle speed | KPH {MPH}