PID/DATA MONITOR TABLE [BCM]

id0902f5345900

—: Not applicable

PID name | Unit/Operation | Data contents | Inspection item(s)
--- | --- | --- | ---
BRK_FLUID | Normal/Low | • Brake fluid level above MIN: Normal • Brake fluid level below MIN: Low | Brake fluid level sensor
CCNT_GEM | — | • DTCs detected: 1—255 • No DTCs detected: 0 | Perform the DTC inspection.
CLS_LOCK | Off/Lock | • Any door open: Off • All doors closed: Lock | Door lock switches (lock)
DRSW_D | Close/OPEN | • Front door (driver-side) closed: Close • Front door (driver-side) open: OPEN | Front door switch (driver-side)
DRSW_P | Close/OPEN | • Front door (passenger-side) closed: Close • Front door (passenger-side) open: OPEN | Front door switch (passenger-side)
DRSW_REAR | Close/OPEN | • Rear door closed: Close • Rear door open: OPEN | Rear door switch
HAZARD | Off/On | • Hazard warning switch turned off: Off • Hazard warning switch turned on: On | Hazard warning switch
HOOD_SW*1 | Close/OPEN | • Bonnet closed: Close • Bonnet open: OPEN Note • “CLOSE” is displayed on vehicles with the theft-deterrent system. | Bonnet latch switch
LLSW_D | Unlock/Lock | • Driver-side lock knob unlocked: Unlock • Driver-side lock knob locked: Lock | Front door lock-link switch (driver-side)
PRK_BRK | Off/On | • Parking brake not depressed (Parking brake switch in the off position): Off • Parking brake depressed (Parking brake switch in the on position): On | Parking brake switch
RWASH_SW | Off/On | • Rear washer switch in the off position: Off • Rear washer switch in the on position: On | Rear washer switch
T_GATE_SW | Close/OPEN | • Liftgate closed: Close • Liftgate open: OPEN | Liftgate latch switch
TURN_SW_L | Off/On | • Turn switch is in the off position: Off • Turn switch is in the LEFT position: On | Turn switch
TURN_SW_R | Off/On | • Turn switch is in the off position: Off • Turn switch is in the RIGHT position: On | Turn switch
WPINT_REAR | Off/On | • Rear wiper switch is in the OFF position: Off • Rear wiper switch is in the INT position: On | Rear wiper switch

*1 :With theft-deterrent system