TRANSMISSION/TRANSAXLE TECHNICAL DATA

id055000800100

Automatic Transaxle [AY6A-EL, AY6AX-EL]

Item | Specification
--- | ---
ATF | Type | JWS3309
Capacity (approx. quantity) | 6.6 L {7.0 US qt, 5.8 lmp qt}

Line pressure

Test Condition | Specification (kPa {kgf/cm2, psi})
--- | ---
Idle | D position | 335—505 {3.42—5.14, 48.6—73.2}
R position | 495—705 {5.05—7.18, 71.8—102.0}

Stall speed

Test Condition | Specification (rpm)
--- | ---
R position | 2,555
D position | 2,637

Time lag

Test Condition | Specification (s)
--- | ---
From N position to D position | 1.5 s or less
From N position to R position