BLIND SPOT MONITORING (BSM) BRACKET REMOVAL/INSTALLATION [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE]

id0922008105e2

1. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [MZI-3.7].)

2. Remove the rear combination light. (See REAR COMBINATION LIGHT REMOVAL/INSTALLATION.)

3. Remove the rear bumper. (See REAR BUMPER REMOVAL/INSTALLATION.)

4. Remove the BSM control module. (See BLIND SPOT MONITORING (BSM) CONTROL MODULE REMOVAL/INSTALLATION [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)

5. Remove the nuts.

ac9uuw00004939

6. Remove the BSM bracket.

7. Install in the reverse order of removal.