OUTER MIRROR GLASS REMOVAL

id091200002800

1. Press area A of the mirror glass so that area B moves outward.

ac9wzw00001662

2. Detach pin A while lifting up the inside of the mirror glass holder.

ac9wzw00001663

3. Pull the mirror glass holder and remove pins B.

4. Disconnect the heated outer mirror connectors. (vehicles with heated outer mirrors)

5. Remove the mirror glass holder and the outer mirror glass as a single unit.