CYLINDER HEAD CONSTRUCTION [MZI-3.7]

id0110c5100300

• A high-heat conductive, lightweight aluminum alloy cylinder head has been adopted.
• Compact, pentroof-type combustion chambers have been adopted.
• Torque-to-yield cylinder head bolts have been adopted for the cylinder head bolts.
• The boss for installing the camshaft position (CMP) sensor is provided at the rear of the cylinder head.

ac9wzn00000702