CLOCK SPRING INSPECTION

id081000802200

1. Verify that the continuity is as indicated in the table.

  • If not as indicated in the table, replace the clock spring.

With INFO Switch

  Note
  • When the vehicle-side connector for the clock spring is disconnected, terminals 1A and 1B are shorted to prevent unexpected operation (deployment) of the air bag module.

ac9wzw00002951

ac9wzw00002952

Without INFO Switch

  Note
  • When the vehicle-side connector for the clock spring is disconnected, terminals 1C and 1D are shorted to prevent unexpected operation (deployment) of the air bag module.

ac9wzw00002953

ac9wzw00002954