Bluetooth UNIT FUNCTION

id092000843200

• The Bluetooth unit communicates information between the Bluetooth-enabled device and the vehicle’s audio/information display. The profile is used for communication between the Bluetooth unit and Bluetooth-enabled unit. The CAN system is used for communication between the Bluetooth unit and the vehicle’s audio/information display.
• The Bluetooth unit sends/receives information by using the common profile with the Bluetooth-enabled device. If they do not have the same profile, communication is impossible. In this case, the functions requiring the profile are disabled.
• The Bluetooth unit uses the following profiles:

Profiles | Function
--- | ---
A2DP 1.0/1.2 (Advanced audio distribution profile) | Sends/receives music or audio data.
AVRCP1.0/1.3/1.4 (Audio/video remote control profile) | Sends/receives operation information.
HFP1.0/1.5 (Hands-free profile) | Enables a call using a hands-free phone.
OPP 1.1 (Object push profile) | Phone book can be downloaded.
PBAP1.0 (Phone book access profile) | Sends/receives phone book data.

• The Bluetooth unit is equipped with a voice recognition function that allows the user to operate the Bluetooth-enabled mobile phone using voice. It also has a learning function to improve the precision of voice recognition.
• The Bluetooth unit has a self-diagnostic function to facilitate malfunction diagnosis.
• The Bluetooth system has the following functions:

Voice Recognition Function

• The voice commands are pre-set for the Bluetooth unit. When the voice spoken into the vehicle’s microphone matches the voice command, the Bluetooth unit performs the mode set to the voice command.

Learning Voice Recognition Function

• Phrases for learning voice recognition are pre-set for the Bluetooth unit. The Bluetooth unit recognizes the features of the user’s voice comparing them with the pre-set phrase to improve the precision of the voice recognition.

TTG (Text to Grammar) function

• This function matches the voice of the user to the phone book text data. Calls can be made just by downloading a Bluetooth-enabled mobile phone book without having to re-register using the voice recognition mode.

Speed dial function (Favorites registration function)

• The speed dial function can used to register frequently called contacts to the speed dial enabling phone calls to be made with little operation. Phone numbers and names registered beforehand are displayed on the speed dial screen to enable immediate phone calling. A maximum of 8 phone numbers can be registered.

  Note
  • For the phone number registration method, refer to the owner's manual.

Self-diagnostic Function

• The Bluetooth unit performs self-diagnosis to detect a malfunctioning part.
• Refer to the ON-BOARD DIAGNOSTIC SYSTEM FUNCTION [Bluetooth SYSTEM (HANDS-FREE TELEPHONE (HF/TEL) SYSTEM)] for the self-diagnosis.