SEAT WARMER UNIT REMOVAL/INSTALLATION

id091300802400

Removal

  Warning
  • Handling a front seat (with built-in side air bag) improperly can accidentally operate (deploy) the air bag, which may seriously injure you. Read the service warnings before handling a front seat (with built-in side air bag). (See AIR BAG SYSTEM SERVICE WARNINGS.) (See AIR BAG SYSTEM SERVICE CAUTIONS.)

  Caution
  • After removing a front seat, do not operate the slider lever. If the slider lever is operated, the left and right slide positions will deviate, and the slide adjuster may be damaged after the front seat is installed.
  • Verify that there are no malfunctions in the sliding mechanism after installing a front seat.
  • When performing the procedure with a front seat removed from the vehicle, perform the procedure on a clean rag so as not to damage or soil the seat.

1. Switch the ignition to off.

2. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [MZI-3.7].)

3. Disconnect the negative battery cable and wait 1 min or more.

4. Remove the following parts:

  (1) Front seat (See FRONT SEAT REMOVAL/INSTALLATION.)

  (2) Front seat side cover (See FRONT SEAT SIDE COVER REMOVAL/INSTALLATION.)

  (3) Front seat front cover (See FRONT SEAT FRONT COVER REMOVAL/INSTALLATION.)

  (4) Front seat back trim (See FRONT SEAT BACK TRIM REMOVAL/INSTALLATION.)

  (5) Front seat cushion trim (See FRONT SEAT CUSHION TRIM REMOVAL/INSTALLATION.)

5. Peel off the seat warmer unit from the position of the arrow shown in the figure.

ac9uuw00003611

  Caution
  • There is a possibility for it to become impossible to reused when seat pad are damaged.Carefully remove the spacer pad glued onto the seat pad.

  ac9uuw00003612

Installation

  Note
  • If there are any peel-off marks from the seat back pad and seat cushion pad remaining after they have been peeled off, the seat pad cannot be reused and it must be newly replaced.

  ac9uuw00003613

1. Stick the seat warmer unit onto the seat pad shown in the figure.

ac9uuw00003614

2. Install the following parts:

  (1) Front seat cushion trim (See FRONT SEAT CUSHION TRIM REMOVAL/INSTALLATION.)

  (2) Front seat back trim (See FRONT SEAT BACK TRIM REMOVAL/INSTALLATION.)

  (3) Front seat front cover (See FRONT SEAT FRONT COVER REMOVAL/INSTALLATION.)

  (4) Front seat side cover (See FRONT SEAT SIDE COVER REMOVAL/INSTALLATION.)

  (5) Front seat (See FRONT SEAT REMOVAL/INSTALLATION.)

3. Connect the negative battery cable.

4. Inspect the seat warmer unit. (See SEAT WARMER UNIT INSPECTION.)