REAR MOUNT CAMERA INSPECTION

id092000815000

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Liftgate upper trim (See LIFTGATE UPPER TRIM REMOVAL/INSTALLATION.)

  (2) Liftgate side trim (See LIFTGATE SIDE TRIM REMOVAL/INSTALLATION.)

  (3) Liftgate lower trim (See LIFTGATE LOWER TRIM REMOVAL/INSTALLATION.)

  (4) Rear finisher (See REAR FINISHER REMOVAL/INSTALLATION.)

  (5) Rear mount camera (See REAR MOUNT CAMERA REMOVAL/INSTALLATION.)

3. Prepare four dry cell batteries (1.5 V)

4. Connect the four dry cell batteries in a series.

ac5wzw00005108

5. Connect the positive pole of the dry cell battery to rear mount camera terminal A, and the negative pole to terminal E.

ac5wzw00004640

6. With the cell batteries being connected, measure the waveform between rear mount camera terminal C and terminal B.

7. Verify that waveform A shown in the figure is displayed two times or more.

ac9wzw00002991

8. If the voltage is not as shown in the figure, replace the rear mount camera.