No.5 DOOR GLASS STOPS BEFORE FULLY OPENING/CLOSING [POWER WINDOW SYSTEMS (EXTERIOR OPEN/CLOSE FUNCTION)]

id090361809000

5 | Door glass stops before fully opening/closing
POSSIBLE CAUSE | • Power window main switch malfunction • Power window subswitch malfunction • Power window motor malfunction • Battery malfunction (low voltage) • Door glass improper installation • Power window initialization procedure error • Keyless control module malfunction • BCM malfunction • Keyless entry system signal reception error (outside operation area, radio signal interference)

Diagnostic Procedure

Step | Inspection | Action
--- | --- | ---
1 | • Operate the door glass in auto/manual by operating the power window main switch/power window subswitch. • Does the door glass stop before fully opening/closing using either operation? | Yes | Inspect the following parts, and repair or replace. • Power window main switch (See POWER WINDOW MAIN SWITCH INSPECTION.) • Power window subswitch (See POWER WINDOW SUBSWITCH INSPECTION.) • Power window motor (See POWER WINDOW MOTOR INSPECTION.) • Battery (Low voltage) • Door glass (Installation condition)
No | Go to the next step.
2 | • Inspect the operation of the door glass by repeating Step 1 above. • Does the door glass stop before fully opening/closing while in auto operation? | Yes | Perform the power window initialization procedure. (See POWER WINDOW SYSTEM INITIALIZATION PROCEDURE.)
No | Go to the next step.
3 | • Open the door glass by operating the transmitter. • Does the door glass stop before fully opening? | Yes | Inspect the following parts, and repair or replace. • Keyless control module (See KEYLESS CONTROL MODULE INSPECTION [ADVANCED KEYLESS ENTRY AND START SYSTEM].) • BCM (See BODY CONTROL MODULE (BCM) INSPECTION.) • Keyless entry system signal reception error (Outside operation area, radio signal interference.)
No | Go to the next step.
4 | • Close the door glass by operating the transmitter. • Does the door glass stop before fully closing? | Yes | Inspect the following parts, and repair or replace. • Keyless control module (See KEYLESS CONTROL MODULE INSPECTION [ADVANCED KEYLESS ENTRY AND START SYSTEM].) • BCM (See BODY CONTROL MODULE (BCM) INSPECTION.) • Keyless entry system signal reception (the system is in outside operation area and/or influenced radio signal interference intermittently)
No | Reinspect for malfunction recurrence. If the malfunction is not corrected, repeat the procedure from Step 1.