KNOCK SENSOR (KS) INSPECTION [MZI-3.7]

id0140c3802800

Resistance Inspection

1. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [MZI-3.7].)

2. Disconnect the KS connector. (See KNOCK SENSOR (KS) REMOVAL/INSTALLATION [MZI-3.7].)

3. Measure the resistance between the following terminals:

ac9wzw00001734

  • KS terminals A and B (KS (LH))
  • KS terminals C and D (KS (RH))
    ― If not as specified, replace the KS. (See KNOCK SENSOR (KS) REMOVAL/INSTALLATION [MZI-3.7].)

  KS resistance

  Approx. 4.87 Mohms