FLOOR COVERING REMOVAL/INSTALLATION

id091700803000

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Front seat (See FRONT SEAT REMOVAL/INSTALLATION.)

  (2) Second-row seat (See SECOND-ROW SEAT REMOVAL/INSTALLATION.)

  (3) Edge cover (See LONG SLIDER REMOVAL/INSTALLATION.)

  (4) Long slider cover (See LONG SLIDER REMOVAL/INSTALLATION.)

  (5) Trunk box (See TRUNK BOX REMOVAL/INSTALLATION.)

  (6) Seat side box (See SEAT SIDE BOX REMOVAL/INSTALLATION.)

  (7) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)

  (8) Third-row seat (See THIRD-ROW SEAT REMOVAL/INSTALLATION.)

  (9) Dashboard under cover (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

  (10) Front scuff plate inner (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)

  (11) Front side trim (See FRONT SIDE TRIM REMOVAL/INSTALLATION.)

  (12) Dust cover (See STEERING WHEEL AND COLUMN REMOVAL/INSTALLATION.)

  (13) Side wall (See SIDE WALL REMOVAL/INSTALLATION.)

  (14) Console panel (See CONSOLE PANEL REMOVAL/INSTALLATION.)

  (15) Console cover (See CONSOLE COVER REMOVAL/INSTALLATION.)

  (16) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)

  (17) Front console box mat (See FRONT CONSOLE BOX MAT REMOVAL/INSTALLATION.)

  (18) Indicator panel (See INDICATOR PANEL REMOVAL/INSTALLATION.)

  (19) Front console box (See FRONT CONSOLE BOX REMOVAL/INSTALLATION.)

  (20) Console (See CONSOLE REMOVAL/INSTALLATION.)

  (21) Rear scuff plate inner (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)

  (22) Front seat belt lower anchor installation bolt (Driver side) (See FRONT SEAT BELT REMOVAL/INSTALLATION.)

  (23) B-pillar lower trim (See B-PILLAR LOWER TRIM REMOVAL/INSTALLATION.)

  (24) Third-row seat belt lower anchor installation bolt (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (25) Trunk side trim (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)

  (26) Fuel-filler lid release cover (See FUEL-FILLER LID OPENER REMOVAL/INSTALLATION.)

3. Remove the fasteners A and B.

ac9uuw00000596

4. Remove the nut.

5. Take the floor covering out from the opened liftgate.

6. Install in the reverse order of removal.