PID/DATA MONITOR TABLE [FORWARD SENSING CAMERA (FSC)]

id0902p9032600

—: Not applicable

PID | Unit/Operation | Data contents | Inspection item(s)
--- | --- | --- | ---
A_ANG_PITCH | ° (deg) | Displays vanishing point correction angle (pitch) corrected by forward sensing camera (FSC) when performing forward sensing camera (FSC) aiming using M-MDS. | Forward sensing camera (FSC)
A_ANG_ROLL | ° (deg) | Displays vanishing point correction angle (roll) corrected by forward sensing camera (FSC) when performing forward sensing camera (FSC) aiming using M-MDS. | Forward sensing camera (FSC)
A_ANG_YAW | ° (deg) | Displays vanishing point correction angle (yaw) corrected by forward sensing camera (FSC) when performing forward sensing camera (FSC) aiming using M-MDS. | Forward sensing camera (FSC)
BRAKE_SW | Off/On | • Off: Brake switch No.2 is off. (Brake pedal is depressed.) • On: Brake switch No.2 is on. (Brake pedal is not depressed.) | Brake switch
DSP_LANE_ST | Off/Dash_Lane/Solid_Lane | • Off: Vehicle lanes not displayed in LCD display. • Dash_Lane: Displays broken lines in LCD display. • Solid_Lane: Displays actual lanes in LCD display. | LCD display (instrument cluster)
DSP_WRN_ST | Off/LDWS_Left/LDWS_Right/LDWS_Fail/HBC_Fail/Camera_BLK/FOW_Warning/FOW_Fail/FSC_Fail/Camera_DRDT | • Off: Warning not displayed in LCD display. • LDWS_Left: Warning related to lane departure on vehicle left side is displayed in LCD display. • LDWS_Right: Warning related to lane departure on vehicle right side is displayed in LCD display. • LDWS_Fail: Displays “ERROR” in LCD display. • HBC_Fail: Displays “ERROR” in LCD display. • Camera_BLK: Displays “ERROR” in LCD display. • FOW_Warning: Warning related to forward obstruction warning (FOW) system is displayed in LCD display. • FOW_Fail: Displays “ERROR” in LCD display. • FSC_Fail: Displays “ERROR” in LCD display. • Camera_DRDT: Displays “ERROR” in LCD display. | LCD display (instrument cluster)
FOW_LEAD_V | Off/On | • Off: Vehicle ahead not displayed in LCD display. • On: Vehicle ahead displayed in LCD display. | LCD display (instrument cluster)
HBC_H/L_CS | Hi_Request/Low_Request/Invalid | • Hi_Request: HI beam switch signal received. • Low_Request: LO beam switch signal received. • Invalid: Error in HI/LO beam switch request signal | Forward sensing camera (FSC)
IL_ST_HBC | Off/Green_On/Green_Flash/Amber_On/Amber_Flash | • Off: HBC indicator light (green)/HBC warning light (amber) turns off. • Green_On: HBC indicator light (green) is illuminated. • Green_Flash: HBC indicator light (green) is flashing. • Amber_On: HBC warning light (amber) is illuminated. • Amber_Flash: HBC warning light (amber) is flashing. | • HBC indicator light (green) (instrument cluster) • HBC warning light (amber) (instrument cluster)
LDWS_BUZZER | Off/On | • Off: LDWS warning alarm does not sound. • On: LDWS warning alarms sounds. | LDWS warning alarm (instrument cluster)
LDWS_VOLUME | Off/On | • Off: LDWS warning alarm volume request signal is not received. • Low: LDWS warning alarm volume request signal Lo is received. • High: LDWS warning alarm volume request signal Hi is received. | LDWS warning alarm (instrument cluster)
PCS_BUZZER | Off/On | • Off: FOW warning alarm does not sound. • On: FOW warning alarm sounds. | FOW warning alarm (instrument cluster)
RS_SOUND_CS | Off/Left/Right | Note • Displays in the M-MDS but it does not operate.
VPWR_IG1 | V | Displays forward sensing camera (FSC) power supply voltage. | Forward sensing camera (FSC)
VSPD | KPH, MPH | Displays vehicle speed. | —