DTC TABLE [AUTO LIGHT/WIPER CONTROL MODULE]

id0902j1347100

DTC No. | Detection condition | Description | Page
--- | --- | --- | ---
B1014 | • Auto light/wiper control module detects the auto light sensor/rain sensor internal malfunction. | Auto light sensor/rain sensor malfunction | (See DTC B1014 [AUTO LIGHT/WIPER CONTROL MODULE].)
B1317 | • Auto light/wiper control module power supply voltage from the battery is excessively high. | Auto light/wiper control module power supply voltage high input | (See DTC B1317 [AUTO LIGHT/WIPER CONTROL MODULE].)
B1318 | • Auto light/wiper control module power supply voltage from the battery is excessively low. | Auto light/wiper control module power supply voltage low input | (See DTC B1318 [AUTO LIGHT/WIPER CONTROL MODULE].)
B1342 | • Auto light/wiper control module detects the internal ECU malfunction. | Auto light/wiper control module internal ECU malfunction | (See DTC B1342 [AUTO LIGHT/WIPER CONTROL MODULE].)
U0140 | • Auto light/wiper control module cannot receive the signal from the BCM for 5 s or more. | Communication error with BCM | (See DTC U0140 [AUTO LIGHT/WIPER CONTROL MODULE].)
U2030 | • Auto light/wiper control module detects the communication error with the auto light sensor/rain sensor. | Communication error with auto light sensor/rain sensor | (See DTC U2030 [AUTO LIGHT/WIPER CONTROL MODULE].)