FRONT AUTO LEVELING SENSOR INSPECTION

id091800809900

1. Disconnect the negative battery cable.

2. Jack up the vehicle.

3. Remove the splash shield (LH).

4. Remove the front auto leveling sensor. (See FRONT AUTO LEVELING SENSOR REMOVAL/INSTALLATION.)

5. Connect three 1.5 V dry cell batteries in a series.

ac9wzw00002992

6. Connect the positive pole of the battery to front auto leveling sensor terminal C, and the negative pole to terminal A, then apply voltage of 4.5 V between terminals C and A.

7. Connect the tester as shown in the figure.

8. Measure the voltage while the link is moved up and down slowly.

acxwzw00000844

  • If not as indicated in the table, replace the front auto leveling sensor.