SUSPENSION TECHNICAL DATA

id025000800100

Front wheel alignment [2WD] (Unloaded)*1

Item | Fuel gauge indication
--- | ---
Empty | 1/4 | 1/2 | 3/4 | Full
Maximum steering angle [Tolerance ±3°] | Inner | 38°
Outer | 32°
Total toe-in | Tire [Tolerance ±4 {0.16}] | (mm {in}) | 2 {0.08}
Rim inner [Tolerance ±3 {0.12}] | Vehicle equipped with 18 inch wheel: 1.2 {0.047} Vehicle equipped with 20 inch wheel: 1.4 {0.055}
(degree) | 0°09′±0°18′
Caster angle*2[Tolerance ±1°] | 3°01′ | 3°02′ | 3°03′ | 3°04′
Camber angle*2[Tolerance ±1°] | -0°19′ | -0°20′ | -0°21′
Steering axis inclination (Reference value) | 11°31′ | 11°32′ | 11°33′ | 11°34′ | 11°35′

*1 :Engine coolant and engine oil are at specified level. Spare tire, jack and tools are in designated position.
*2 :Difference between left and right must not exceed 1°30′.

Front wheel alignment [4WD] (Unloaded)*1

Item | Fuel gauge indication
--- | ---
Empty | 1/4 | 1/2 | 3/4 | Full
Maximum steering angle [Tolerance ±3°] | Inner | 38°
Outer | 32°
Total toe-in | Tire [Tolerance ±4 {0.16}] | (mm {in}) | 2 {0.08}
Rim inner [Tolerance ±3 {0.12}] | Vehicle equipped with 18 inch wheel: 1.2 {0.047} Vehicle equipped with 20 inch wheel: 1.4 {0.055}
(degree) | 0°09′±0°18′
Caster angle*2[Tolerance ±1°] | 3°02′ | 3°03′ | 3°04′ | 3°05′
Camber angle*2[Tolerance ±1°] | -0°19′ | -0°20′ | -0°21′
Steering axis inclination (Reference value) | 11°31′ | 11°32′ | 11°33′ | 11°34′ | 11°35′

*1 :Engine coolant and engine oil are at specified level. Spare tire, jack and tools are in designated position.
*2 :Difference between left and right must not exceed 1°30′.

Rear wheel alignment [2WD] (Unloaded) *1

Item | Fuel gauge indication
--- | ---
Empty | 1/4 | 1/2 | 3/4 | Full
Total toe-in | Tire [Tolerance ±4 {0.16}] | (mm {in}) | 2 {0.08}
Rim inner [Tolerance ±3 {0.12}] | Vehicle equipped with 18 inch wheel: 1.2 {0.047} Vehicle equipped with 20 inch wheel: 1.4 {0.055}
(degree) | 0°09′±0°18′
Camber angle *2 [Tolerance ±1°] | -0°26′ | -0°27′ | -0°29′ | -0°30′ | -0°32′
Thrust angle (Reference value) [Tolerance ±0°48′] | 0°

*1 :Engine coolant and engine oil are at specified level. Spare tire, jack and tools are in designated position.
*2 :Difference between left and right must not exceed 1°30′.

Rear wheel alignment [4WD] (Unloaded) *1

Item | Fuel gauge indication
--- | ---
Empty | 1/4 | 1/2 | 3/4 | Full
Total toe-in | Tire [Tolerance ±4 {0.16}] | (mm {in}) | 2 {0.08}
Rim inner [Tolerance ±3 {0.12}] | Vehicle equipped with 18 inch wheel: 1.2 {0.047} Vehicle equipped with 20 inch wheel: 1.4 {0.055}
(degree) | 0°09′±0°18′
Camber angle *2 [Tolerance ±1°] | -0°27′ | -0°28′ | -0°30′ | -0°31′ | -0°33′
Thrust angle (Reference value) [Tolerance ±0°48′] | 0°

*1 :Engine coolant and engine oil are at specified level. Spare tire, jack and tools are in designated position.
*2 :Difference between left and right must not exceed 1°30′.

Standard tire

Item | Specification
--- | ---
Tire | Size | 245/60R18 104H | 245/50R20 102V
Air pressure (kPa {bar} <psi>) | Front | 250 {2.5} <36> | 230 {2.3} <33>
Rear
Remaining tread | (mm {in}) | 1.6 {0.07}
Wheel | Size | 18×7 1/2J | 20×7 1/2J
Material | Aluminum alloy
Wheel inset | (mm {in}) | 45 {1.8}
Wheel pitch circle diameter | (mm {in}) | 114.3 {4.5}
Wheel and tire runout | Lateral direction | 2.0 {0.08} max.
(mm {in}) | Radial direction | 1.5 {0.06} max.
Wheel and tire imbalance | (g {oz}) | Adhesive-type*1: 12 {0.42} max. Knock-type*2: 8 {0.28} max. | Adhesive-type*1: 11 {0.39} max. Knock-type*2: 7 {0.25} max.
*1: Do not install three or more weights. Do not affix the weights such that they are parallel to each other or overlapping. The total weight of all the weights is 160 g {5.64 oz} or less. *2: Do not install three or more weights. One weight is 60 g {2.1 oz} or less and two weights are 100 g {3.53 oz} or less.
Wheel nut tightening torque | (N·m {kgf·m, ft·lbf}) | 107.8—147.0 {11.0—14.9, 79.6—108.4}

Spare tire

Item | Specification
--- | ---
Tire | Size | 195/80R17 99M
Air pressure (kPa {bar} <psi>) | 250 {2.5} <36>
Remaining tread | (mm {in}) | 1.6 {0.07}
Wheel | Size | 17×5 1/2J
Material | Steel
Wheel inset | (mm {in}) | 45 {1.8}
Wheel pitch circle diameter | (mm {in}) | 114.3 {4.5}
Wheel and tire runout | Lateral direction | 2.5 {0.09} max.
(mm {in}) | Radial direction | 2.0 {0.07} max.
Wheel nut tightening torque | (N·m {kgf·m, ft·lbf}) | 107.8—147.0 {11.0—14.9, 79.6—108.4}

Suspension

Item | Specification
--- | ---
Front lower arm rotational torque | 2.62 N·m {26.7 kgf·cm, 23.1 in·lbf} max.
Front stabilizer control link ball joint starting torque | 0.2—2.0 N·m {3—20 kgf·cm, 2—17 in·lbf}
Rear stabilizer control link ball joint starting torque | 0.2—2.0 N·m {3—20 kgf·cm, 2—17 in·lbf}