DIFFERENTIAL OIL TEMPERATURE SENSOR REMOVAL/INSTALLATION

id031800805700

  Warning
  • Hot differential oil may cause severe burns. Do not perform maintenance while differential oil is hot.

1. Disconnect the differential oil temperature sensor connector.

2. Remove the differential oil temperature sensor.

ac9uuw00001905

3. Apply differential oil to the O-ring.

4. Install the differential oil temperature sensor.

  Tightening torque

  12.7—17.3 N·m {1.30—1.76 kgf·m, 9.4—12.7 ft·lbf}

5. Connect the differential oil temperature sensor connector.