LONG SLIDER REMOVAL/INSTALLATION

id091300803100

1. Disconnect the negative battery cable.

2. Remove the second-row seat. (See SECOND-ROW SEAT REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

ac9uuw00000744

1 | Edge cover
2 | Long slider cover

4. Remove the following parts:

  (1) Trunk box (See TRUNK BOX REMOVAL/INSTALLATION.)

  (2) Seat side box (See SEAT SIDE BOX REMOVAL/INSTALLATION.)

  (3) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)

  (4) Third-row seat (See THIRD-ROW SEAT REMOVAL/INSTALLATION.)

  (5) Rear scuff plate inner (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)

  (6) Third-row seat belt lower anchor installation bolt (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (7) Trunk side trim (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)

5. Set the floor covering out of the way.

6. Remove in the order indicated in the table.

ac9wzw00002481

1 | Bolt
2 | Long slider

7. Install in the reverse order of removal.