FRONT DOOR TRIM REMOVAL/INSTALLATION

id091700802500

1. Disconnect the negative battery cable.

2. Remove the inner garnish. (See INNER GARNISH REMOVAL/INSTALLATION.)

3. Open the cover using a small flathead screwdriver and remove the screw.

4. Remove the armrest garnish in the direction of the arrow.

ac9uuw00000853

5. Remove the bolt.

6. Detach clips A from the front door using a fastener remover.

7. Pull the front door trim upward and detach tabs B from the front door.

8. Remove tab A, and move the front door trim in the direction of the arrow.

ac9uuw00000854

9. Turn the inner handle cover in the direction of the arrow and remove it from the front door trim.

ac9uuw00002106

10. Disconnect the power window main switch connector and the power outer mirror switch connector and door lock switch connector. (Driver side)

11. Disconnect the power window subswitch connector. (Passenger side)

12. Disconnect the courtesy light connector.

13. Remove the front door trim.

14. Install in the reverse order of removal.