COUPLING COMPONENT ASSEMBLY

id031800805500

  Warning
  • The engine stand is equipped with a self-lock mechanism, however, if the coupling unit is in a tilted condition, the self-lock mechanism could become inoperative. If the coupling unit unexpectedly rotates it could cause injury, therefore do not maintain the coupling unit in a tilted condition. When turning the coupling unit, grasp the rotation handle firmly.

1. Assemble in the order indicated in the table.

ac9wzw00000847

1 | Coupling unit
2 | Output shaft (See Output Shaft Assembly Note.)
3 | Bearing (See Bearing Assembly Note.)
4 | Snap ring
5 | Coupling case (See Coupling Case Assembly Note.)
6 | Shim
7 | Oil seal (See Oil Seal Assembly Note.)
8 | Companion flange (See Companion Flange Assembly Note.)
9 | Washer
10 | Locknut (See Locknut Assembly Note.)

Output Shaft Assembly Note

1. Install the output shaft to the coupling unit and partially tighten the bolts.

2. Install the companion flange to the output shaft.

3. Secure the companion flange using the SST, and tighten the bolts.

ac9uuw00001839

  Tightening torque

  41.2—53.9 N·m {4.21—5.49 kgf·m, 30.4—39.7 ft·lbf}

Bearing Assembly Note

1. Assemble the bearing to the coupling case using the SSTs.

ac9uuw00001840

Coupling Case Assembly Note

  Caution
  • The coupling unit will be damaged if it is pressed directly by a press. Always press the coupling unit into the coupling case using the SST.

1. Assemble the coupling unit to the coupling case using the SSTs and a press.

ac9uuw00001841

Oil Seal Assembly Note

1. Apply the specified oil to a new oil seal lip.

2. Install the oil seal to the coupling case using the SST.

ac9uuw00001842

Companion Flange Assembly Note

1. Install the coupling case to the SST as shown.

ac9uuw00001843

2. Install the companion flange.

Locknut Assembly Note

1. Secure the companion flange using the SST, and tighten a new locknut.

ac9uuw00001844

  Tightening torque

  167—226 N·m {17.1—23.0 kgf·m, 124—166 ft·lbf}