ADVANCED KEY BATTERY REPLACEMENT [ADVANCED KEYLESS ENTRY AND START SYSTEM]

id0914008156z6

1. Pull out the auxiliary key.

am3uuw00004663

2. Insert a tape-wrapped flathead screwdriver into the notch in the advanced key and rotate it in the direction shown in the figure to open the advanced key.

acxuuw00004006

3. Remove the battery cap.

4. Remove the battery.

acxuuw00004007

  Note
  • If the O-ring has come off, put it back in place before installing the battery.

  am3uuw00004362

5. Install the new battery (CR2025) with the negative pole facing down.

acxuuw00004008

6. Install the battery cap.

7. Align the upper and lower covers and close the transmitter.

acxuuw00004009

8. Insert the auxiliary key.

acxuuw00004010