HIGH-MOUNT BRAKE LIGHT REMOVAL/INSTALLATION

id091800802000

1. Disconnect the negative battery cable.

2. Remove the liftgate upper trim. (See LIFTGATE UPPER TRIM REMOVAL/INSTALLATION.)

3. Remove the rear spoiler. (See REAR SPOILER REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

ac9uuw00000508

1 | Screw
2 | High-mount brake light

5. Install in the reverse order of removal.