DTC P0011:00 [MZI-3.7]

id0102d2700100

DTC P0011:00 | CMP timing over-advanced (RH)
--- | ---
DETECTION CONDITION | • The PCM monitors the variable valve timing position for an over-advanced camshaft timing. The test fails when the camshaft timing exceeds a maximum calibrated value or remains in an advanced position.
POSSIBLE CAUSE | • Spool valve in OCV (RH) is stuck in advanced position • Improper valve timing due to timing chain slippage • OCV (RH) malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record FREEZE FRAME DATA on the repair order, then go to the next step.
2 | VERIFY RELATED SERVICE INFORMATION AVAILABILITY • Verify related Service Information availability. • Is any related Service Information available? | Yes | Perform repair or diagnosis according to the available Service Information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | VERIFY TIMING CHAIN INSTALLATION • Stop the engine. • Remove the front cover. • Is the camshaft timing mark at the correct point? (See TIMING CHAIN REMOVAL/INSTALLATION [MZI-3.7].) | Yes | Go to the next step.
No | Reinstall the timing chain, then go to Step 5.
4 | INSPECT OCV (RH) • Inspect the OCV (RH). (See OIL CONTROL VALVE (OCV) INSPECTION [MZI-3.7].) • Is there any malfunction? | Yes | Replace the OCV (RH), then go to the next step. (See OIL CONTROL VALVE (OCV) REMOVAL/INSTALLATION [MZI-3.7].)
No | Go to the next step.
5 | VERIFY TROUBLESHOOTING OF DTC P0011:00 HAS BEEN COMPLETED • Make sure to reconnect all disconnected connectors. • Clear the DTC from the PCM memory using the M-MDS. • Turn the ignition switch off. • Start the engine and warm it up completely. • Is the same DTC present? | Yes | Repeat the inspection from Step 1. • If the malfunction recurs, replace the PCM. (See PCM REMOVAL/INSTALLATION [MZI-3.7].) Go to the next step.
No | Go to the next step.
6 | VERIFY AFTER REPAIR PROCEDURE • Perform the “AFTER REPAIR PROCEDURE”. (See AFTER REPAIR PROCEDURE [MZI-3.7].) • Are any DTCs present? | Yes | Go to the applicable DTC inspection. (See DTC TABLE [MZI-3.7].)
No | Troubleshooting completed.