FRONT MAP LIGHT INSPECTION

id091800808600

1. Disconnect the negative battery cable.

2. Remove the intruder sensor. (with intruder sensor) (See INTRUDER SENSOR REMOVAL/INSTALLATION.)

3. Remove the front map light. (See FRONT MAP LIGHT REMOVAL/INSTALLATION.)

4. Verify that the continuity between the front map light terminals is as indicated in the table.

ac9wzw00001721

  • If not as indicated in the table, replace the front map light.

ac9wzw00001722

5. Apply battery positive voltage to front map light terminal C, and connect terminal F to ground.

6. Switch the interior light switch to the DOOR position and verify that the front map light illuminates.

  • If the light does not illuminate, replace the map light.