SEAT WARMER SWITCH INSPECTION

id091300801300

  Note
  • Front climate control unit and seat warmer switch are a single unit.

1. Remove the seat warmer switch. (See SEAT WARMER SWITCH REMOVAL/INSTALLATION.)

2. Disconnect the seat warmer switch connector.

3. Inspect for resistance and continuity between the seat warmer switch terminals using a tester. (See FRONT CLIMATE CONTROL UNIT INSPECTION.)