TRANSMITTER BATTERY REPLACEMENT [KEYLESS ENTRY SYSTEM]

id0914008057b3

1. Insert a flathead screwdriver into the transmitter notch and remove the key from the transmitter by pressing the tab.

am3uuw00004386

2. Insert a flathead screwdriver into the transmitter notch and open the transmitter.

abatjw00002557

3. Remove the battery by pressing it in the direction of the arrow shown in the figure.

am3uuw00004387

4. Install the new battery (CR1620) with the plus pole facing down.

abatjw00002974

5. Align the upper and lower covers and close the transmitter.

  Battery type

  Lithium battery CR1620

  Battery life

  Approx. 2 years (when used approx. 10 times/day)

6. Install the key to the transmitter.

  Note
  • When connecting the key to the transmitter, grip the key and the transmitter as shown in the figure and connect until a click sound is heard.
  • If the key is not completely connected to the transmitter, they may come apart.

  am3uuw00002762