WINDSHIELD WIPER MOTOR DISASSEMBLY/ASSEMBLY

id091900801000

1. Disassemble in the order indicated in the table.

ac9wzw00001035

1 | Screw
2 | Windshield wiper motor (See Windshield Wiper Motor Assembly Note.)
3 | Wiper link No. 1 (See Ball Joint Assembly Note.)
4 | Wiper link No. 2 (See Ball Joint Assembly Note.)
5 | Main link (See Ball Joint Assembly Note.)

2. Assemble in the reverse order of disassembly.

Ball Joint Assembly Note

1. Use a clean cloth to protect the link, and squeeze using pliers.

ac9wzw00001590

Windshield Wiper Motor Assembly Note

1. Connect the windshield wiper motor to the vehicle wiring harness connector, operate the windshield wipers, and then stop them at the auto-stop position.

2. Adjust the motor crank and wiper link No.1 so that they are parallel as shown in the figure.

ac9wzw00001034

3. Assemble the windshield wiper motor.