DTC TABLE [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE]

id0902q3960500

BSM Control Module (LH)

×: Applicable
—: Not applicable

DTC No. | BSM OFF indicator light | Description | Fail-safe function | Drive cycle | Self test type*1 | Memory function | Page
--- | --- | --- | --- | --- | --- | --- | ---
B118C:11 | Flash | BSM indicator light (LH) circuit malfunction | × | — | C, D | × | (See DTC B118C:11 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)
B118C:15 | Flash | BSM indicator light (LH) circuit malfunction | × | — | C, D | × | (See DTC B118C:15 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)
U0010:88 | Flash | Module communication error (MS-CAN) | × | — | C, D | × | (See DTC U0010:88/U0100:00/U0140:00/U0155:00 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)
U0100:00 | Flash | Communication error with PCM | × | — | C, D | ×
U0140:00 | Flash | Communication error with BCM | × | — | C, D | ×
U0155:00 | Flash | Communication error with instrument cluster | × | — | C, D | ×
U0233:00 | Flash | Communication error with BSM control module (RH) | × | — | C, D | × | (See DTC U0233:00 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)
U0401:68 | Flash | Error signal received from PCM | × | — | C, D | × | (See DTC U0401:68 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)
U0422:68 | Flash | Error signal received from BCM | × | — | C, D | × | (See DTC U0422:68 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)
U3000:01 | Flash | Electrical malfunction inside BSM control module | × | — | C, D | × | (See DTC U3000:01 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)
U3000:09 | Flash | BSM control module internal malfunction | × | — | C, D | × | (See DTC U3000:09 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)
U3000:4A | Flash | BSM OFF switch circuit malfunction | × | — | C, D | × | (See DTC U3000:4A [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)
U3000:54 | Flash | Radar performance malfunction | × | — | C, D | × | (See DTC U3000:54 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)
U3000:97 | Flash | Radar performance malfunction | × | — | C, D | × | (See DTC U3000:97 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)
U3003:04 | Flash | Instrument cluster configuration error | × | — | C, D | × | (See DTC U3003:04 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)
U3003:16 | Flash | BSM control module low power supply voltage input (less than 8.2 V) | × | — | C, D | × | (See DTC U3003:16 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)
U3003:17 | Flash | BSM control module high power supply voltage input (16.8 V or more) | × | — | C, D | × | (See DTC U3003:17 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)

*1 :C: CMDTC self test, D: ODDTC self test

BSM Control Module (RH)

×: Applicable
—: Not applicable

DTC No. | BSM OFF indicator light | Description | Fail-safe function | Drive cycle | Self test type*1 | Memory function | Page
--- | --- | --- | --- | --- | --- | --- | ---
B118D:11 | Flash | BSM indicator light (RH) circuit malfunction | × | — | C, D | × | (See DTC B118D:11 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)
B118D:15 | Flash | BSM indicator light (RH) circuit malfunction | × | — | C, D | × | (See DTC B118D:15 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)
U0010:88 | Flash | Module communication error (MS-CAN) | × | — | C, D | × | (See DTC U0010:88/U0100:00/U0140:00/U0155:00 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)
U0100:00 | Flash | Communication error with PCM | × | — | C, D | ×
U0140:00 | Flash | Communication error with BCM | × | — | C, D | ×
U0155:00 | Flash | Communication error with instrument cluster | × | — | C, D | ×
U0232:00 | Flash | Communication error with BSM control module (LH) | × | — | C, D | × | (See DTC U0232:00 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)
U0401:68 | Flash | Error signal received from PCM | × | — | C, D | × | (See DTC U0401:68 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)
U0422:68 | Flash | Error signal received from BCM | × | — | C, D | × | (See DTC U0422:68 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)
U3000:01 | Flash | Electrical malfunction inside BSM control module | × | — | C, D | × | (See DTC U3000:01 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)
U3000:09 | Flash | BSM control module internal malfunction | × | — | C, D | × | (See DTC U3000:09 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)
U3000:54 | Flash | Radar performance malfunction | × | — | C, D | × | (See DTC U3000:54 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)
U3000:97 | Flash | Radar performance malfunction | × | — | C, D | × | (See DTC U3000:97 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)
U3003:04 | Flash | Instrument cluster configuration error | × | — | C, D | × | (See DTC U3003:04 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)
U3003:16 | Flash | BSM control module low power supply voltage input (less than 8.2 V) | × | — | C, D | × | (See DTC U3003:16 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)
U3003:17 | Flash | BSM control module high power supply voltage input (16.8 V or more) | × | — | C, D | × | (See DTC U3003:17 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)

*1 :C: CMDTC self test, D: ODDTC self test