REAR DOOR MODULE PANEL REMOVAL/INSTALLATION

id091100520900

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Inner sail garnish (See INNER SAIL GARNISH REMOVAL/INSTALLATION).

  (2) Rear door trim (See REAR DOOR TRIM REMOVAL/INSTALLATION.)

  (3) Rear door speaker (See REAR DOOR SPEAKER REMOVAL/INSTALLATION.)

  (4) Rear door glass (See REAR DOOR GLASS REMOVAL/INSTALLATION.)

3. Remove the clips securing the wiring harness shown in the figure and set the wiring harness out of the way.

ac9wzw00000853

4. Remove screws and fastener.

ac9wzw00000854

5. Remove the rear door module panel.

6. Install in the reverse order of removal.