QUICK RELEASE CONNECTOR CONSTRUCTION/OPERATION [MZI-3.7]

id0114d2151400

Quick Release Connector Position

ac9wzn00000288

Construction

• An SST is not used with this type.
• Mainly consists of a retainer and O-ring. The quick release connector is integrated with the joint port and therefore cannot be disassembled.
• When the quick release connector is connected, the fuel pipe projection is locked at the clamp lock point. To release the quick connector lock for each type, follow the procedure in the order shown in each figure.

ac9wzn00000671