INSTRUMENT CLUSTER CONFIGURATION

id092200800300

  Note
  • Use the IDS (laptop PC) because the PDS (Pocket PC) does not support the INSTRUMENT CLUSTER CONFIGURATION.

1. Connect the M-MDS to DLC-2.

ac9uuw00000570

2. After the vehicle is identified, select the following items from the initial screen of the M-MDS.

  1. Select “Module Programming”.

3. Then, select items from the screen menu in the following order.

  1. Select "Programmable Module Installation".
  2. Select "IC".

4. Perform the configuration according to the directions on the screen.

5. Retrieve DTCs by the M-MDS, then verify that there is no DTC present.