TCS OFF SWITCH REMOVAL/INSTALLATION

id041800817400

1. Remove the dashboard under cover. (See DASHBOARD REMOVAL/INSTALLATION.)

2. Remove the bonnet release lever. (See BONNET LATCH AND RELEASE LEVER REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

L.H.D.

ac9wzw00000840

1 | TCS OFF switch (See TCS OFF Switch Removal Note.)
2 | TCS OFF switch connector

R.H.D.

ac9wzw00000841

1 | TCS OFF switch (See TCS OFF Switch Removal Note.)
2 | TCS OFF switch connector

4. Install in the reverse order of removal.

TCS OFF Switch Removal Note

1. Access the TCS OFF switch from behind of the dashboard, and squeeze the tabs of the switch.

2. Remove the TCS OFF switch from the dashboard.