CRANKSHAFT POSITION (CKP) SENSOR REMOVAL/INSTALLATION [MZI-3.7]

id0140c3800600

  Note
  • Disconnect the connector after the CKP sensor is removed to prevent the CKP sensor from falling off.
  • The bolt and sensor are integrated and cannot be pulled out.
  • When removing the CKP sensor, be careful not to drop the tool.
  • The bolt and sensor must be pulled in different directions. Pull them as indicated in the figure.

  ac9wzw00001729

1. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [MZI-3.7].)

2. Remove the following parts for easier access:

  1. HO2S (LH) (See HEATED OXYGEN SENSOR (HO2S) REMOVAL/INSTALLATION [MZI-3.7].)
  2. WU-TWC (LH) bracket (L type) (See EXHAUST SYSTEM REMOVAL/INSTALLATION [MZI-3.7].)
  3. WU-TWC (LH) (See EXHAUST SYSTEM REMOVAL/INSTALLATION [MZI-3.7].)

3. Remove in the order indicated in the table.

ac9wzw00001730

1 | Insulator
2 | Cover
3 | CKP sensor
4 | CKP sensor connector

4. Install in the reverse order of removal.