PID/DATA MONITOR TABLE [THEFT-DETERRENT SYSTEM]

id0902g7960700

Foreword

1. When the theft-deterrent control module switches to the alert mode, it stores the related theft-deterrent control module control status data.

2. Stored data up to the previous two times can be checked using the PID/data monitor function.

PID name (Definition) | Unit/Operation | Data contents | Inspection item(s)
--- | --- | --- | ---
DRSW_D | Close/OPEN | • Close: Front door (driver-side) is closed. • OPEN: Front door (driver-side) is opened. | Front door switch (driver-side)
DRSW_P | Close/OPEN | • Close: Front door (passenger-side) is closed. • OPEN: Front door (passenger-side) is opened. | Front door switch (passenger-side)
DRSW_REAR | Close/OPEN | • Close: Rear door is closed. • OPEN: Rear door is opened. | Rear door switch
HOOD_SW | Close/OPEN | • Close: Bonnet is closed. • OPEN: Bonnet is opened. | Bonnet latch switch
LLSW_D | Unlock/Lock | • Unlock: Driver's door lock knob unlocked. • Lock: Driver's door lock knob locked. | Front door lock-link switch (driver-side)
LLSW_P+R | Unlock/Lock | • Unlock: Door lock knob other than driver's door unlocked. • Lock: Door lock knob other than driver's door locked. | • Front door lock-link switch (passenger-side) • Rear door lock-link switch (LH) • Rear door lock-link switch (RH)
T_GATE_SW | Close/OPEN | • Close: Liftgate is closed. • OPEN: Liftgate is opened. | Liftgate latch switch
VPWR | V | Indicates the theft-deterrent control module power supply voltage. | Battery