AUTO-DIMMING MIRROR REMOVAL/INSTALLATION

id091200099900

With Forward Sensing Camera (FSC)

1. Disconnect the negative battery cable.

2. Remove the cover. (See FORWARD SENSING CAMERA (FSC) REMOVAL/INSTALLATION.)

3. Disconnect the auto-dimming mirror connector.

ac9wzw00002980

4. Remove the screw.

ac9wzw00002981

5. Remove the auto-dimming mirror in the direction of arrow shown in the figure.

ac9wzw00002982

6. Install in the reverse order of removal.

Without Forward Sensing Camera (FSC)

Removal

1. Disconnect the negative battery cable.

2. Insert a tape-wrapped flathead screwdriver into the notch and pry with the screwdriver in the direction shown by the arrow to remove the covers.

ac9wzw00003014

3. Remove the covers.

ac9wzw00003015

4. Remove the rain sensor. (See RAIN SENSOR REMOVAL/INSTALLATION.)

5. Disconnect the auto-dimming mirror connector.

ac9wzw00001676

6. Make a tool as shown in the figure using wire.

ac9wzw00001677

  Caution
  • Using the tool with bare hands can cause injury. Always wear gloves when using the tool.
  • To prevent damage to the lens, do not use a flathead screwdriver.

7. Insert the tool to the position shown in the figure and press the center part of the spring.

ac9wzw00001678

  Caution
  • Perform the procedure while being careful not to damage the lens.

8. Pull out the auto-dimming mirror toward the vehicle rear.

ac9wzw00001679

  Caution
  • When removing the auto-dimming mirror, it may hit the headliner and cause a damage. Hold the auto-dimming mirror with hands and be careful not to contact it with the headliner.

Installation

1. Install the auto-dimming mirror onto the base.

ac9wzw00001680

2. Connect the auto-dimming mirror connector.

3. Install the rain sensor. (See RAIN SENSOR REMOVAL/INSTALLATION.)

4. Install the covers.

ac9wzw00003016