SELECTOR CABLE ADJUSTMENT

id051800800700

1. Remove the center console.

2. Shift the selector lever to P position.

3. Unlock the lock piece of the selector cable (selector lever side) in the order shown in the figure.

L.H.D.

ac9wzw00000017

R.H.D.

ac9wzw00000018

4. Verify that the manual shaft is in P position.

5. Lock the lock piece of the selector cable (selector lever side) in the order shown in the figure.

L.H.D.

ac9wzw00000019

R.H.D.

ac9wzw00000020

6. Install the center console.

7. Shift the selector lever from P position to M range, and make sure that there are no other components in that area to interfere with the lever.