DTC TABLE [INSTRUMENT CLUSTER]

id0902e8347100

×: Applicable
—: Not applicable

DTC No. | Detection condition | Description | Freeze frame data | Page
--- | --- | --- | --- | ---
B1213*1 | • Only one key is registered | Only one key ID number is registered | — | (See SECURITY LIGHT: 21, DTC: B1213/P1260/P1260:00 [IMMOBILIZER SYSTEM (KEYLESS ENTRY SYSTEM)].)
B1342 | • Instrument cluster detects the internal ECU malfunction. | Instrument cluster internal ECU malfunction | — | (See DTC B1342 [INSTRUMENT CLUSTER].)
B1600*1 | • The key ID number data cannot be read | The key ID number data cannot be read | — | (See SECURITY LIGHT: 13, DTC: B1600/P1260/P1260:00 [IMMOBILIZER SYSTEM (KEYLESS ENTRY SYSTEM)].)
B1601*1 | • The instrument cluster has detected unregistered key ID number | The instrument cluster has detected unregistered key ID number | — | (See SECURITY LIGHT: 15, DTC: B1601/P1260/P1260:00 [IMMOBILIZER SYSTEM (KEYLESS ENTRY SYSTEM)].)
B1602*1 | • The instrument cluster cannot read key ID number data normally | The instrument cluster cannot read key ID number data normally | — | (See SECURITY LIGHT: 14, DTC: B1602/P1260/P1260:00 [IMMOBILIZER SYSTEM (KEYLESS ENTRY SYSTEM)].)
B1681*1 | • No detected communication with the coil antenna | No detected communication with the coil antenna | — | (See SECURITY LIGHT: 11, DTC: B1681/P1260/P1260:00 [IMMOBILIZER SYSTEM (KEYLESS ENTRY SYSTEM)].)
B2103*1 | • Coil antenna malfunction • The PCM determined a malfunction in the coil antenna even though it is normal | • Coil antenna malfunction • The PCM determined a malfunction in the coil antenna even though it is normal | — | (See SECURITY LIGHT: 12, DTC: B2103/P1260/P1260:00 [IMMOBILIZER SYSTEM (KEYLESS ENTRY SYSTEM)].)
B2139*1 | • ID number data in the instrument cluster and the PCM are different | ID number data in the PCM and the instrument cluster do not match | — | (See SECURITY LIGHT: 23, DTC: B2139/P1260/P1260:00 [IMMOBILIZER SYSTEM (KEYLESS ENTRY SYSTEM)].)
B2141*1 | • Communication error between the instrument cluster and the PCM (data transfer error) | Communication error between the instrument cluster and the PCM (data transfer error) | — | (See SECURITY LIGHT: 22, DTC: B2141/P1260/P1260:00 [IMMOBILIZER SYSTEM (KEYLESS ENTRY SYSTEM)].)
B2143*2 | • Two or more codes are overlapping. | ID registration failure | — | (See DTC B2143.)
B2431*1 | • Key ID number registration error | Key ID number registration error | — | (See SECURITY LIGHT: 13, DTC: B2431/P1260/P1260:00 [IMMOBILIZER SYSTEM (KEYLESS ENTRY SYSTEM)].)
B2477 | • Instrument cluster configuration has not been correctly performed. | Instrument cluster configuration error | — | (See DTC B2477 [INSTRUMENT CLUSTER].)
B2868*2 | • The instrument cluster receives error signals from the wheel unit. | Wheel unit No.1 (internal malfunction) | — | (See DTC B2868, B2869, B2870, B2871.)
B2869*2 | • The instrument cluster receives error signals from the wheel unit. | Wheel unit No.2 (internal malfunction) | —
B2870*2 | • The instrument cluster receives error signals from the wheel unit. | Wheel unit No.3 (internal malfunction) | —
B2871*2 | • The instrument cluster receives error signals from the wheel unit. | Wheel unit No.4 (internal malfunction) | —
U0073 | • Instrument cluster detects a CAN bus communication line (HS-CAN) malfunction. | Module communication error (HS-CAN) | — | (See FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].) (See FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (R.H.D.)].)
U0100 | • Instrument cluster cannot receive the CAN signal from the PCM. | Communication error with PCM | ×
U0101 | • Instrument cluster cannot receive the CAN signal from the TCM. | Communication error with TCM | ×
U0114*3 | • Instrument cluster cannot receive the CAN signal from the 4WD control module. | Communication error with 4WD control module | ×
U0121 | • Instrument cluster cannot receive the CAN signal from the DSC/RSC HU/CM. | Communication error with DSC/RSC HU/CM | ×
U0127*2 | With advanced keyless entry and start system: • The instrument cluster cannot receive signal from the keyless control module. With keyless entry system • The instrument cluster cannot receive signal from the keyless receiver. | With advanced keyless entry and start system: • Communication failure between instrument cluster and keyless control module With keyless entry system • Communication failure between instrument cluster and keyless receiver | × | (See DTC U0127.)
U0140 | • Instrument cluster cannot receive the CAN signal from the BCM. | Communication error with BCM | × | (See FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].) (See FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (R.H.D.)].)
U0151 | • Instrument cluster cannot receive the CAN signal from the SAS control module. | Communication error with SAS control module | ×
U0200*4 | • Instrument cluster cannot receive the CAN signal from the BSM control module. | Communication error with BSM control module | ×
U0214*5 | • Instrument cluster cannot receive the CAN signal from the keyless control module. | Communication error with keyless control module | ×
U023A*6 | • Instrument cluster cannot receive the CAN signal from the forward sensing camera (FSC). | Communication error with forward sensing camera (FSC) | ×
U2023 | • Instrument cluster cannot receive the correct data from the keyless control module. (Vehicles with advanced keyless entry and start system) • Instrument cluster cannot receive the correct data from the PCM. | Error data from other module | × | (See DTC U2023 [INSTRUMENT CLUSTER].)
U2064 | • Instrument cluster receives the warning light illumination request signal. | Warning light illumination request signal from other module | × | (See DTC U2064 [INSTRUMENT CLUSTER].)
U2197 | • Instrument cluster receives the invalid vehicle speed from the PCM under the following conditions: ― Passed 20 s after turn the ignition switch to the ON position ― Odometer is normal and more than 30 km {19 mile}. ― Battery voltage is more than 10 V. ― Received invalid data from the PCM for 0.5 s. | Error signal from PCM | — | (See DTC U2197 [INSTRUMENT CLUSTER].)
U2510*1 | • Communication error between the instrument cluster and the PCM (no response) | Communication error between the instrument cluster and the PCM (no response) | — | (See SECURITY LIGHT: 16, DTC: U2510/P1260/P1260:00 [IMMOBILIZER SYSTEM (KEYLESS ENTRY SYSTEM)].)
U2616*2 | • The keyless receiver has continuously not received a signal from the wheel unit for a certain period. | Wheel unit No.1 (No response) | × | (See DTC U2616, U2617, U2618, U2619.)
U2617*2 | • The keyless receiver has continuously not received a signal from the wheel unit for a certain period. | Wheel unit No.2 (No response) | ×
U2618*2 | • The keyless receiver has continuously not received a signal from the wheel unit for a certain period. | Wheel unit No.3 (No response) | ×
U2619*2 | • The keyless receiver has continuously not received a signal from the wheel unit for a certain period. | Wheel unit No.4 (No response) | ×

*1 :Vehicles with keyless entry system
*2 :Vehicles with tire pressure monitoring system
*3 :4WD
*4 :Vehicles with blind spot monitoring (BSM)
*5 :Vehicles with advanced keyless entry and start system
*6 :Vehicles with forward sensing camera (FSC)