INSTRUMENT CLUSTER STRUCTURAL VIEW

id092200101200

Meter and Gauge

Without forward sensing camera (FSC)

ac9wzn00000746

With FSC

ac9wzn00000747

Warning and Indicator Light

Without FSC

ac9wzn00000748

×: Applicable

No. | Warning and indicator light | Input signal source | CAN system | Description | Note
--- | --- | --- | --- | --- | ---
1 | 120 km/h warning light | PCM | × | If the vehicle speed exceeds 120 km/h, the vehicle speed warning light illuminates. | With 120 km/h warning light
2 | Headlight auto leveling warning light | Auto leveling control module | — | The headlight auto leveling system warning light illuminates if a malfunction in the auto leveling system is detected. | —
3 | Keyless indicator light (green) | Keyless control module | × | When the start knob can be turned (unlocked), the keyless indicator light (green) illuminates when the start knob is pressed in. (See ADVANCED KEYLESS ENTRY SYSTEM FUNCTION.) | With advanced keyless system
Keyless warning light (red) | The keyless control module illuminates the keyless warning light (red) when the advanced keyless system has a malfunction. (See ADVANCED KEYLESS ENTRY SYSTEM FUNCTION.)
4 | Tire pressure monitoring system warning light | DSC/RSC HU/CM | — | When the front fog light illuminates, the front fog light indicator light illuminates. | With TPMS
5 | Generator warning light | PCM | × | Illuminates if the generator output is not normal. (See GENERATOR CONSTRUCTION [MZI-3.7].) | —
6 | Electronic throttle control (ETC) warning light | PCM | × | Illuminates if an abnormality occurs with the parts related to the electronic throttle body. (See ON-BOARD DIAGNOSTIC SYSTEM TEST MODE [MZI-3.7].) | —
7 | BSM OFF indicator light | BSM control module | × | • If the BSM is malfunctioning, the BSM OFF light flashes. (See BLIND SPOT MONITORING (BSM) ON-BOARD DIAGNOSTIC FUNCTION [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].) (See ON-BOARD DIAGNOSTIC [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].) • When the BSM OFF switch is pressed to disable, the BSM OFF light illuminates. (See BLIND SPOT MONITORING (BSM) OFF INDICATOR LIGHT CONSTRUCTION/OPERATION [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].) (See BLIND SPOT MONITORING (BSM) OFF INDICATOR LIGHT [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].) | With BSM
8 | AT warning light | TCM | × | The AT warning light illuminates to alert the driver of a malfunction in the automatic transaxle. (See AT WARNING LIGHT CONSTRUCTION/OPERATION [AY6A-EL, AY6AX-EL].) | —
9 | Turn indicator light | BCM | × | When the turn light illuminates, the turn indicator light illuminates. | —
10 | High-beam indicator light | Headlight (HI) | — | When the headlight (high-beam) illuminates, the high-beam indicator light illuminates. | —
11 | DSC indicator light | DSC/RSC HU/CM | × | • If the DSC/RSC system is malfunctioning, the DSC indicator light remains illuminated. (See ON-BOARD DIAGNOSTIC SYSTEM FUNCTION.) • When the RSC or DSC or TCS is operating, the DSC indicator light flashes. (See DSC INDICATOR LIGHT OPERATION.) | —
12 | Door ajar warning light | BCM | × | When any door or the liftgate is open, the door ajar warning light illuminates. | —
13 | Air bag system warning light | SAS control module | × | SAS control module illuminates the air bag system warning light if the SRS air bag system has a malfunction. (See ON-BOARD DIAGNOSTIC FUNCTION.) | —
14 | Security light | • PCM (Without advanced keyless system) • Keyless control module (With advanced keyless system) | × | The PCM (without advanced keyless system) or the keyless control module (with advanced keyless system) illuminates the security light if the immobilizer system has a malfunction. (See SECURITY LIGHT CONSTRUCTION/OPERATION.) | —
15 | Seat belt warning light | SAS control module | × | When the driver′s seat belt is not fastened, the seat belt warning light illuminates. | —
16 | Washer fluid level warning light | BCM | × | When the washer fluid-level is low, the washer fluid level warning light illuminates. (See WASHER FLUID-LEVEL SENSOR FUNCTION.) | —
17 | Rear fog indicator light | Rear fog light relay | — | When the rear fog light illuminates, the rear fog light indicator light illuminates. | With rear fog light
18 | Cruise main indicator light (amber) | PCM | × | Illuminates if the cruise control system is in control status. (See CRUISE CONTROL SYSTEM OUTLINE [MZI-3.7].) | —
Cruise set indicator light (green)
19 | 4WD warning light | 4WD control module | × | If the 4WD system is malfunctioning, the 4WD warning light remains illuminated. If the 4WD system control is temporarily suspended due to the rear differential oil temperature becoming abnormally hot or a related cause, the warning light flashes. (See 4WD WARNING LIGHT CONSTRUCTION.) | 4WD
20 | Oil pressure warning light | BCM | × | Illuminates if the oil pressure is low. | —
21 | Selector indicator light | TCM | × | Displays the selector lever position. (See SELECTOR INDICATOR LIGHT CONSTRUCTION/OPERATION [AY6A-EL, AY6AX-EL].) | —
22 | Gear position indicator light | TCM | × | Displays the gear position when in the M range. (See SELECTOR INDICATOR LIGHT CONSTRUCTION/OPERATION [AY6A-EL, AY6AX-EL].) | —
23 | MIL | PCM | × | Illuminates if a malfunction occurs in the engine control system and automatic transaxle control system. (See ON-BOARD DIAGNOSTIC SYSTEM MALFUNCTION DISPLAY FUNCTION [MZI-3.7].) | —
24 | Brake system warning light | DSC/RSC HU/CM | × | If the DSC/RSC system is malfunctioning, the brake system warning light remains illuminated. (See ON-BOARD DIAGNOSTIC SYSTEM FUNCTION.) | —
BCM | × | • When the brake fluid-level is low, the brake system warning light illuminates. • When the parking brake is operating, the brake system warning light illuminates. | —
25 | Front fog indicator light | Front fog light relay | — | When the front fog light illuminates, the front fog light indicator light illuminates. | —
26 | TCS OFF light | DSC/RSC HU/CM | × | • If the DSC/RSC system is malfunctioning, the TCS OFF light remains illuminated. (See ON-BOARD DIAGNOSTIC SYSTEM FUNCTION.) • When the TCS OFF switch is pressed to disable, the TCS OFF light illuminates. (See TCS OFF SWITCH, TCS OFF LIGHT OPERATION.) | —
27 | TNS indicator light | TNS relay | — | When the TNS illuminates, the TNS indicator light illuminates. | —
28 | ABS warning light | DSC/RSC HU/CM | × | If the DSC/RSC system is malfunctioning, the ABS warning light remains illuminated. (See ON-BOARD DIAGNOSTIC SYSTEM FUNCTION.) | —
29 | Fuel-level warning light | Fuel gauge sender unit | — | When the remaining fuel amount in the fuel tank is low, the fuel-level warning light illuminates. | —

With FSC

ac9wzn00000749

×: Applicable

No. | Warning and indicator light | Input signal source | CAN system | Description | Note
--- | --- | --- | --- | --- | ---
1 | Headlight auto leveling warning light | Auto leveling control module | — | The headlight auto leveling system warning light illuminates if a malfunction in the auto leveling system is detected. | —
2 | 120 km/h warning light | PCM | × | If the vehicle speed exceeds 120 km/h, the vehicle speed warning light illuminates. | With 120 km/h warning light
3 | MIL | PCM | × | Illuminates if a malfunction occurs in the engine control system and automatic transaxle control system. (See ON-BOARD DIAGNOSTIC SYSTEM MALFUNCTION DISPLAY FUNCTION [MZI-3.7].) | —
4 | Tire pressure monitoring system warning light | DSC/RSC HU/CM | — | When the front fog light illuminates, the front fog light indicator light illuminates. | With TPMS
5 | Door ajar warning light | BCM | × | When any door or the liftgate is open, the door ajar warning light illuminates. | —
6 | Air bag system warning light | SAS control module | × | SAS control module illuminates the air bag system warning light if the SRS air bag system has a malfunction. (See ON-BOARD DIAGNOSTIC FUNCTION.) | —
7 | Generator warning light | PCM | × | Illuminates if the generator output is not normal. (See GENERATOR CONSTRUCTION [MZI-3.7].) | —
8 | Electronic throttle control (ETC) warning light | PCM | × | Illuminates if an abnormality occurs with the parts related to the electronic throttle body. (See ON-BOARD DIAGNOSTIC SYSTEM TEST MODE [MZI-3.7].) | —
9 | AT warning light | TCM | × | The AT warning light illuminates to alert the driver of a malfunction in the automatic transaxle. (See AT WARNING LIGHT CONSTRUCTION/OPERATION [AY6A-EL, AY6AX-EL].) | —
10 | Turn indicator light | BCM | × | When the turn light illuminates, the turn indicator light illuminates. | —
11 | High-beam indicator light | Headlight (HI) | — | When the headlight (high-beam) illuminates, the high-beam indicator light illuminates. | —
12 | DSC indicator light | DSC/RSC HU/CM | × | • If the DSC/RSC system is malfunctioning, the DSC indicator light remains illuminated. (See ON-BOARD DIAGNOSTIC SYSTEM FUNCTION.) • When the RSC or DSC or TCS is operating, the DSC indicator light flashes. (See DSC INDICATOR LIGHT OPERATION.) | —
13 | Selector indicator light | TCM | × | Displays the selector lever position. (See SELECTOR INDICATOR LIGHT CONSTRUCTION/OPERATION [AY6A-EL, AY6AX-EL].) | —
14 | Gear position indicator light | TCM | × | Displays the gear position when in the M range. (See SELECTOR INDICATOR LIGHT CONSTRUCTION/OPERATION [AY6A-EL, AY6AX-EL].) | —
15 | Security light | • PCM (Without advanced keyless system) • Keyless control module (With advanced keyless system) | × | The PCM (without advanced keyless system) or the keyless control module (with advanced keyless system) illuminates the security light if the immobilizer system has a malfunction. (See SECURITY LIGHT CONSTRUCTION/OPERATION.) | —
16 | Washer fluid level warning light | BCM | × | When the washer fluid-level is low, the washer fluid level warning light illuminates. (See WASHER FLUID-LEVEL SENSOR FUNCTION.) | —
17 | Keyless indicator light (green) | Keyless control module | × | When the start knob can be turned (unlocked), the keyless indicator light (green) illuminates when the start knob is pressed in. (See ADVANCED KEYLESS ENTRY SYSTEM FUNCTION.) | With advanced keyless system
Keyless warning light (red) | The keyless control module illuminates the keyless warning light (red) when the advanced keyless system has a malfunction. (See ADVANCED KEYLESS ENTRY SYSTEM FUNCTION.)
18 | Brake system warning light | DSC/RSC HU/CM | × | If the DSC/RSC system is malfunctioning, the brake system warning light remains illuminated. (See ON-BOARD DIAGNOSTIC SYSTEM FUNCTION.) | —
BCM | × | • When the brake fluid-level is low, the brake system warning light illuminates. • When the parking brake is operating, the brake system warning light illuminates. | —
19 | BSM OFF indicator light | BSM control module | × | • If the BSM is malfunctioning, the BSM OFF light flashes. (See BLIND SPOT MONITORING (BSM) ON-BOARD DIAGNOSTIC FUNCTION [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].) (See ON-BOARD DIAGNOSTIC [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].) • When the BSM OFF switch is pressed to disable, the BSM OFF light illuminates. (See BLIND SPOT MONITORING (BSM) OFF INDICATOR LIGHT CONSTRUCTION/OPERATION [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].) (See BLIND SPOT MONITORING (BSM) OFF INDICATOR LIGHT [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].) | With BSM
20 | TCS OFF light | DSC/RSC HU/CM | × | • If the DSC/RSC system is malfunctioning, the TCS OFF light remains illuminated. (See ON-BOARD DIAGNOSTIC SYSTEM FUNCTION.) • When the TCS OFF switch is pressed to disable, the TCS OFF light illuminates. (See TCS OFF SWITCH, TCS OFF LIGHT OPERATION.) | —
21 | ABS warning light | DSC/RSC HU/CM | × | If the DSC/RSC system is malfunctioning, the ABS warning light remains illuminated. (See ON-BOARD DIAGNOSTIC SYSTEM FUNCTION.) | —
22 | High beam control (HBC) system indicator light (green)/high beam control system (hbc) warning light (amber) | FSC | × | • The HBC indicator light (green) notifies the driver that the High beam control (HBC) system is operating. (See HBC INDICATOR LIGHT (GREEN)/HBC WARNING LIGHT (AMBER).) • The HBC warning light (amber) warns the driver that a malfunction is occurring in the HBC system. (See HBC INDICATOR LIGHT (GREEN)/HBC WARNING LIGHT (AMBER).) | —
23 | Cruise main indicator light (amber) | PCM | × | Illuminates if the cruise control system is in control status. (See CRUISE CONTROL SYSTEM OUTLINE [MZI-3.7].) | —
Cruise set indicator light (green)
24 | TNS indicator light | TNS relay | — | When the TNS illuminates, the TNS indicator light illuminates. | —
25 | Seat belt warning light | SAS control module | × | When the driver′s seat belt is not fastened, the seat belt warning light illuminates. | —
26 | Rear fog indicator light | Rear fog light relay | — | When the rear fog light illuminates, the rear fog light indicator light illuminates. | With rear fog light
27 | 4WD warning light | 4WD control module | × | If the 4WD system is malfunctioning, the 4WD warning light remains illuminated. If the 4WD system control is temporarily suspended due to the rear differential oil temperature becoming abnormally hot or a related cause, the warning light flashes. (See 4WD WARNING LIGHT CONSTRUCTION.) | 4WD
28 | Oil pressure warning light | BCM | × | Illuminates if the oil pressure is low. | —
29 | Front fog indicator light | Front fog light relay | — | When the front fog light illuminates, the front fog light indicator light illuminates. | —
30 | Fuel-level warning light | Fuel gauge sender unit | — | When the remaining fuel amount in the fuel tank is low, the fuel-level warning light illuminates. | —