SELECTOR LEVER STRUCTURE

id051800100400

M Range Switch

Outline

  • The M range switch detects the selector lever in M range position and sends a manual mode request signal to the TCM.

L.H.D.

ac9uun00000328

R.H.D.

ac9wzn00000002

Operation

  • The M range switch is an on/off type switch that turns on when the selector lever is shifted to the M range. It also remains on during up-shift and down-shift operations.

Up Switch

Outline

  • The up switch detects an up-shift operation in the M range and sends an up-shift request signal to the TCM.

L.H.D.

ac9uun00000329

R.H.D.

ac9wzn00000003

Operation

  • The up switch is an on/off type switch that turns on when the selector lever is in the M range (+) side position.

Down Switch

Outline

  • The down switch detects a down-shift operation in the M range and sends a down-shift request signal to the TCM.

L.H.D.

ac9uun00000330

R.H.D

ac9wzn00000004

Operation

  • The down switch is an on/off type switch that turns on when the selector lever is in the M range (–) side position.