DTC P1288:00 [MZI-3.7]

id0102d2317100

DTC P1288:00 | CHT sensor out of self-test range
--- | ---
DETECTION CONDITION | • Indicates the CHT sensor is out of self-test range. The engine is not at a normal operating temperature.
POSSIBLE CAUSE | • Cold engine • Engine overheating • Low engine coolant level • CHT sensor malfunction • Connector or terminal malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record FREEZE FRAME DATA on the repair order, then go to the next step.
2 | VERIFY RELATED SERVICE INFORMATION AVAILABILITY • Verify related Service Information availability. • Is any related Service Information available? | Yes | Perform repair or diagnosis according to the available Service Information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | VERIFY RELATED PENDING CODE OR STORED DTC • Verify the related PENDING CODE or stored DTCs. • Are other DTCs present? | Yes | Go to appropriate DTC inspection. (See DTC TABLE [MZI-3.7].)
No | Go to the next step.
4 | INSPECT THE COOLING SYSTEM • Inspect the vehicle coolant level. • Is the cooling system normal? | Yes | Go to the next step.
No | Inspect the cooling system (overheat), the go to Step 7.
5 | INSPECT CHT SENSOR • Inspect the CHT sensor. (See CYLINDER HEAD TEMPERATURE (CHT) SENSOR INSPECTION [MZI-3.7].) • Is there any malfunction? | Yes | Replace the CHT sensor, then go to Step 7.
No | Go to the next step.
6 | INSPECT FOR CORRECT PCM OPERATION • Disconnect all the PCM connectors. • Visually inspect for: ― Pushed out pins ― Corrosion • Connect all the PCM connectors and verify that they seat correctly. • Retrieve DTCs using the M-MDS. • Is the PENDING CODE for this DTC present? | Yes | Go to the next step.
No | The system is correctly. Go to the next step.
7 | VERIFY TROUBLESHOOTING OF DTC P1288:00 HAS BEEN COMPLETED • Verify that all disconnected connectors reconnected. • Clear the DTC from the PCM memory using the M-MDS. • Perform the KOEO or KOER self-test. (See KOEO/KOER SELF TEST [MZI-3.7].) • Is the PENDING CODE for the DTC present? | Yes | Repeat the inspection from Step 1. • If the malfunction recurs, replace the PCM. (See PCM REMOVAL/INSTALLATION [MZI-3.7].) Go to the next step.
No | Go to the next step.
8 | VERIFY AFTER REPAIR PROCEDURE • Perform the “AFTER REPAIR PROCEDURE”. (See AFTER REPAIR PROCEDURE [MZI-3.7].) • Are any DTCs present? | Yes | Go to the applicable DTC inspection. (See DTC TABLE [MZI-3.7].)
No | Troubleshooting completed.