POWER OUTER MIRROR SWITCH INSPECTION

id091200003400

Mirror Glass Adjustment Switch, Left/right Selection Switch

1. Disconnect the negative battery cable.

2. Remove the power window main switch. (See POWER WINDOW MAIN SWITCH REMOVAL/INSTALLATION.)

  Note
  • The mirror glass adjustment switch, left/right selection switch is integrated with the power window main switch.

3. Verify that the resistance between the mirror glass adjustment switch, left/right selection switch terminals is as indicated in the table.

  • If not as indicated in the table, replace the power window main switch. (See POWER WINDOW MAIN SWITCH REMOVAL/INSTALLATION.)

With position memory system

ac9wzw00002994

Without position memory system

ac9wzw00002995

Retractable Outer Mirror Switch

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Dashboard under cover (Driver side) (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

  (2) Bonnet release lever (See BONNET LATCH AND RELEASE LEVER REMOVAL/INSTALLATION.)

  (3) Retractable outer mirror switch (See POWER OUTER MIRROR SWITCH REMOVAL/INSTALLATION.)

3. Verify that the continuity is as indicated in the table.

ac9wzw00002986

  • If not as indicated in the table, replace the retractable outer mirror switch. (See POWER OUTER MIRROR SWITCH REMOVAL/INSTALLATION.)

ac9wzw00002987

4. Apply battery voltage to retractable outer mirror switch terminal B, and connect terminal A to ground.

5. Verify that the LED illuminates.

  • If there is any malfunction, replace the retractable outer mirror switch. (See POWER OUTER MIRROR SWITCH REMOVAL/INSTALLATION.)