REARVIEW MIRROR REMOVAL

id091200004900

With Auto Light/wiper System

1. Disconnect the negative battery cable.

2. Insert a tape-wrapped flathead screwdriver into the notch and pry with the screwdriver in the direction shown by the arrow to remove the covers.

ac9wzw00001683

3. Remove the covers.

ac9wzw00001684

4. Remove the rain sensor. (See RAIN SENSOR REMOVAL/INSTALLATION.)

5. Make a tool as shown in the figure using wire.

ac9wzw00001685

  Caution
  • Using the tool with bare hands can cause injury. Always wear gloves when using the tool.
  • To prevent damage to the lens sensor, do not use a screwdriver.

6. Insert the tool to the position shown in the figure and press the center part of the spring in the direction of arrows (1), and then pull out the rearview mirror toward in the direction of arrows (2) shown in the figure.

ac9wzw00001686

  Caution
  • Perform the procedure while being careful not to damage the lens.
  • When removing the rearview mirror, it may hit the headliner and cause a damage. Hold the rearview mirror with hands and be careful not to contact it with the headliner.

Without Auto Light/wiper System

1. Insert a flathead screwdriver between the mirror and the base.

ac9wzw00001687

2. Insert the flathead screwdriver to the position shown in the figure and press the center part of the spring.

3. Remove the rearview mirror in the direction of the arrow.

  Caution
  • When removing the rearview mirror, the mirror may hit the top sealing, possibly damaging it. Therefore, hold the mirror body securely by hand when removing the rear view mirror so that the mirror does not contact it.